From cddecd92d1ec2fd05ed1123455e7c6cf6906b5a5 Mon Sep 17 00:00:00 2001
From: YueHaibing <yuehaibing@huawei.com>
Date: Wed, 24 Jul 2019 22:12:01 +0800
Subject: [PATCH] brcmfmac: remove set but not used variable 'dtim_period'

Fixes gcc '-Wunused-but-set-variable' warning:

drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c: In function brcmf_update_bss_info:
drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c:2962:5: warning: variable dtim_period set but not used [-Wunused-but-set-variable]
drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c: In function brcmf_update_bss_info:
drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c:2961:6: warning: variable beacon_interval set but not used [-Wunused-but-set-variable]

They are never used so can be removed.

Reported-by: Hulk Robot <hulkci@huawei.com>
Signed-off-by: YueHaibing <yuehaibing@huawei.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 .../net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c   | 8 +-------
 1 file changed, 1 insertion(+), 7 deletions(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
@@ -2985,8 +2985,6 @@ static s32 brcmf_update_bss_info(struct
 	struct brcmf_pub *drvr = cfg->pub;
 	struct brcmf_bss_info_le *bi;
 	const struct brcmf_tlv *tim;
-	u16 beacon_interval;
-	u8 dtim_period;
 	size_t ie_len;
 	u8 *ie;
 	s32 err = 0;
@@ -3010,12 +3008,9 @@ static s32 brcmf_update_bss_info(struct
 
 	ie = ((u8 *)bi) + le16_to_cpu(bi->ie_offset);
 	ie_len = le32_to_cpu(bi->ie_length);
-	beacon_interval = le16_to_cpu(bi->beacon_period);
 
 	tim = brcmf_parse_tlvs(ie, ie_len, WLAN_EID_TIM);
-	if (tim)
-		dtim_period = tim->data[1];
-	else {
+	if (!tim) {
 		/*
 		* active scan was done so we could not get dtim
 		* information out of probe response.
@@ -3027,7 +3022,6 @@ static s32 brcmf_update_bss_info(struct
 			bphy_err(drvr, "wl dtim_assoc failed (%d)\n", err);
 			goto update_bss_info_out;
 		}
-		dtim_period = (u8)var;
 	}
 
 update_bss_info_out:
