From 078c6a1cbd4cd7496048786beec2e312577bebbf Mon Sep 17 00:00:00 2001
From: Pawel Dembicki <paweldembicki@gmail.com>
Date: Tue, 11 Jan 2022 23:11:32 +0100
Subject: [PATCH 1/1] net: qmi_wwan: add ZTE MF286D modem 19d2:1485
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Modem from ZTE MF286D is an Qualcomm MDM9250 based 3G/4G modem.

T:  Bus=02 Lev=01 Prnt=01 Port=00 Cnt=01 Dev#=  3 Spd=5000 MxCh= 0
D:  Ver= 3.00 Cls=00(>ifc ) Sub=00 Prot=00 MxPS= 9 #Cfgs=  1
P:  Vendor=19d2 ProdID=1485 Rev=52.87
S:  Manufacturer=ZTE,Incorporated
S:  Product=ZTE Technologies MSM
S:  SerialNumber=MF286DZTED000000
C:* #Ifs= 7 Cfg#= 1 Atr=80 MxPwr=896mA
A:  FirstIf#= 0 IfCount= 2 Cls=02(comm.) Sub=06 Prot=00
I:* If#= 0 Alt= 0 #EPs= 1 Cls=02(comm.) Sub=02 Prot=ff Driver=rndis_host
E:  Ad=82(I) Atr=03(Int.) MxPS=   8 Ivl=32ms
I:* If#= 1 Alt= 0 #EPs= 2 Cls=0a(data ) Sub=00 Prot=00 Driver=rndis_host
E:  Ad=81(I) Atr=02(Bulk) MxPS=1024 Ivl=0ms
E:  Ad=01(O) Atr=02(Bulk) MxPS=1024 Ivl=0ms
I:* If#= 2 Alt= 0 #EPs= 2 Cls=ff(vend.) Sub=ff Prot=ff Driver=option
E:  Ad=83(I) Atr=02(Bulk) MxPS=1024 Ivl=0ms
E:  Ad=02(O) Atr=02(Bulk) MxPS=1024 Ivl=0ms
I:* If#= 3 Alt= 0 #EPs= 3 Cls=ff(vend.) Sub=ff Prot=ff Driver=option
E:  Ad=85(I) Atr=03(Int.) MxPS=  10 Ivl=32ms
E:  Ad=84(I) Atr=02(Bulk) MxPS=1024 Ivl=0ms
E:  Ad=03(O) Atr=02(Bulk) MxPS=1024 Ivl=0ms
I:* If#= 4 Alt= 0 #EPs= 3 Cls=ff(vend.) Sub=ff Prot=ff Driver=option
E:  Ad=87(I) Atr=03(Int.) MxPS=  10 Ivl=32ms
E:  Ad=86(I) Atr=02(Bulk) MxPS=1024 Ivl=0ms
E:  Ad=04(O) Atr=02(Bulk) MxPS=1024 Ivl=0ms
I:* If#= 5 Alt= 0 #EPs= 3 Cls=ff(vend.) Sub=ff Prot=ff Driver=qmi_wwan
E:  Ad=88(I) Atr=03(Int.) MxPS=   8 Ivl=32ms
E:  Ad=8e(I) Atr=02(Bulk) MxPS=1024 Ivl=0ms
E:  Ad=0f(O) Atr=02(Bulk) MxPS=1024 Ivl=0ms
I:* If#= 6 Alt= 0 #EPs= 2 Cls=ff(vend.) Sub=42 Prot=01 Driver=usbfs
E:  Ad=05(O) Atr=02(Bulk) MxPS=1024 Ivl=0ms
E:  Ad=89(I) Atr=02(Bulk) MxPS=1024 Ivl=0ms

Signed-off-by: Pawel Dembicki <paweldembicki@gmail.com>
Acked-by: Bjørn Mork <bjorn@mork.no>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/usb/qmi_wwan.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/net/usb/qmi_wwan.c
+++ b/drivers/net/usb/qmi_wwan.c
@@ -1319,6 +1319,7 @@ static const struct usb_device_id produc
 	{QMI_FIXED_INTF(0x19d2, 0x1426, 2)},	/* ZTE MF91 */
 	{QMI_FIXED_INTF(0x19d2, 0x1428, 2)},	/* Telewell TW-LTE 4G v2 */
 	{QMI_FIXED_INTF(0x19d2, 0x1432, 3)},	/* ZTE ME3620 */
+	{QMI_FIXED_INTF(0x19d2, 0x1485, 5)},	/* ZTE MF286D */
 	{QMI_FIXED_INTF(0x19d2, 0x2002, 4)},	/* ZTE (Vodafone) K3765-Z */
 	{QMI_FIXED_INTF(0x2001, 0x7e16, 3)},	/* D-Link DWM-221 */
 	{QMI_FIXED_INTF(0x2001, 0x7e19, 4)},	/* D-Link DWM-221 B1 */
