From 1231481bdb45114abe7b0348c78a943642fde717 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Wed, 8 Apr 2020 11:59:39 +0100
Subject: [PATCH] overlays: Fix dtc warnings in i2c-gpio

Better late than never.

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm/boot/dts/overlays/i2c-gpio-overlay.dts | 3 +++
 1 file changed, 3 insertions(+)

--- a/arch/arm/boot/dts/overlays/i2c-gpio-overlay.dts
+++ b/arch/arm/boot/dts/overlays/i2c-gpio-overlay.dts
@@ -9,6 +9,9 @@
 		target-path = "/";
 
 		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
 			i2c_gpio: i2c@0 {
 				reg = <0xffffffff>;
 				compatible = "i2c-gpio";
