From f32bc2aa01edcba2f2ed5db151cf183eac9ef919 Mon Sep 17 00:00:00 2001
From: Abhimanyu Vishwakarma <Abhimanyu.Vishwakarma@imgtec.com>
Date: Sat, 25 Feb 2017 16:42:50 +0000
Subject: mtd: nor: support mtd name from device tree

Signed-off-by: Abhimanyu Vishwakarma <Abhimanyu.Vishwakarma@imgtec.com>
---
 drivers/mtd/spi-nor/spi-nor.c | 8 +++++++-
 1 file changed, 7 insertions(+), 1 deletion(-)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -4937,6 +4937,7 @@ int spi_nor_scan(struct spi_nor *nor, co
 	struct mtd_info *mtd = &nor->mtd;
 	struct device_node *np = spi_nor_get_flash_node(nor);
 	struct spi_nor_flash_parameter *params = &nor->params;
+	const char __maybe_unused *of_mtd_name = NULL;
 	int ret;
 	int i;
 
@@ -4999,7 +5000,12 @@ int spi_nor_scan(struct spi_nor *nor, co
 	/* Init flash parameters based on flash_info struct and SFDP */
 	spi_nor_init_params(nor);
 
-	if (!mtd->name)
+#ifdef CONFIG_MTD_OF_PARTS
+	of_property_read_string(np, "linux,mtd-name", &of_mtd_name);
+#endif
+	if (of_mtd_name)
+		mtd->name = of_mtd_name;
+	else if (!mtd->name)
 		mtd->name = dev_name(dev);
 	mtd->priv = nor;
 	mtd->type = MTD_NORFLASH;
--- a/drivers/mtd/mtdcore.c
+++ b/drivers/mtd/mtdcore.c
@@ -778,6 +778,17 @@ out_error:
  */
 static void mtd_set_dev_defaults(struct mtd_info *mtd)
 {
+#ifdef CONFIG_MTD_OF_PARTS
+	const char __maybe_unused *of_mtd_name = NULL;
+	struct device_node *np;
+
+	np = mtd_get_of_node(mtd);
+	if (np && !mtd->name) {
+		of_property_read_string(np, "linux,mtd-name", &of_mtd_name);
+		if (of_mtd_name)
+			mtd->name = of_mtd_name;
+	} else
+#endif
 	if (mtd->dev.parent) {
 		if (!mtd->owner && mtd->dev.parent->driver)
 			mtd->owner = mtd->dev.parent->driver->owner;
