From 50edd53c26177e95995533b7d649801086a52f6c Mon Sep 17 00:00:00 2001
From: Claudiu Beznea <claudiu.beznea@microchip.com>
Date: Mon, 11 Oct 2021 14:27:07 +0300
Subject: [PATCH 236/247] clk: at91: sama7g5: add securam's peripheral clock

Add SECURAM's peripheral clock.

Signed-off-by: Claudiu Beznea <claudiu.beznea@microchip.com>
Acked-by: Nicolas Ferre <nicolas.ferre@microchip.com>
Link: https://lore.kernel.org/r/20211011112719.3951784-4-claudiu.beznea@microchip.com
Signed-off-by: Stephen Boyd <sboyd@kernel.org>
---
 drivers/clk/at91/sama7g5.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/clk/at91/sama7g5.c
+++ b/drivers/clk/at91/sama7g5.c
@@ -377,6 +377,7 @@ static const struct {
 	u8 id;
 } sama7g5_periphck[] = {
 	{ .n = "pioA_clk",	.p = "mck0", .id = 11, },
+	{ .n = "securam_clk",	.p = "mck0", .id = 18, },
 	{ .n = "sfr_clk",	.p = "mck1", .id = 19, },
 	{ .n = "hsmc_clk",	.p = "mck1", .id = 21, },
 	{ .n = "xdmac0_clk",	.p = "mck1", .id = 22, },
