From bfa2ba7d9e6b20aca82b99e6842fe18842ae3a0f Mon Sep 17 00:00:00 2001
From: Christian Lamparter <chunkeey@gmail.com>
Date: Fri, 17 May 2019 23:15:57 +0200
Subject: [PATCH 13/15] crypto: crypto4xx - fix AES CTR blocksize value

This patch fixes a issue with crypto4xx's ctr(aes) that was
discovered by libcapi's kcapi-enc-test.sh test.

The some of the ctr(aes) encryptions test were failing on the
non-power-of-two test:

kcapi-enc - Error: encryption failed with error 0
kcapi-enc - Error: decryption failed with error 0
[FAILED: 32-bit - 5.1.0-rc1+] 15 bytes: STDIN / STDOUT enc test (128 bits):
original file (1d100e..cc96184c) and generated file (e3b0c442..1b7852b855)
[FAILED: 32-bit - 5.1.0-rc1+] 15 bytes: STDIN / STDOUT enc test (128 bits)
(openssl generated CT): original file (e3b0..5) and generated file (3..8e)
[PASSED: 32-bit - 5.1.0-rc1+] 15 bytes: STDIN / STDOUT enc test (128 bits)
(openssl generated PT)
[FAILED: 32-bit - 5.1.0-rc1+] 15 bytes: STDIN / STDOUT enc test (password):
original file (1d1..84c) and generated file (e3b..852b855)

But the 16, 32, 512, 65536 tests always worked.

Thankfully, this isn't a hidden hardware problem like previously,
instead this turned out to be a copy and paste issue.

With this patch, all the tests are passing with and
kcapi-enc-test.sh gives crypto4xx's a clean bill of health:
 "Number of failures: 0" :).

Cc: stable@vger.kernel.org
Fixes: 98e87e3d933b ("crypto: crypto4xx - add aes-ctr support")
Fixes: f2a13e7cba9e ("crypto: crypto4xx - enable AES RFC3686, ECB, CFB and OFB offloads")
Signed-off-by: Christian Lamparter <chunkeey@gmail.com>
Signed-off-by: Herbert Xu <herbert@gondor.apana.org.au>
---
 drivers/crypto/amcc/crypto4xx_core.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/crypto/amcc/crypto4xx_core.c
+++ b/drivers/crypto/amcc/crypto4xx_core.c
@@ -1244,7 +1244,7 @@ static struct crypto4xx_alg_common crypt
 			.cra_flags = CRYPTO_ALG_NEED_FALLBACK |
 				CRYPTO_ALG_ASYNC |
 				CRYPTO_ALG_KERN_DRIVER_ONLY,
-			.cra_blocksize = AES_BLOCK_SIZE,
+			.cra_blocksize = 1,
 			.cra_ctxsize = sizeof(struct crypto4xx_ctx),
 			.cra_module = THIS_MODULE,
 		},
@@ -1264,7 +1264,7 @@ static struct crypto4xx_alg_common crypt
 			.cra_priority = CRYPTO4XX_CRYPTO_PRIORITY,
 			.cra_flags = CRYPTO_ALG_ASYNC |
 				CRYPTO_ALG_KERN_DRIVER_ONLY,
-			.cra_blocksize = AES_BLOCK_SIZE,
+			.cra_blocksize = 1,
 			.cra_ctxsize = sizeof(struct crypto4xx_ctx),
 			.cra_module = THIS_MODULE,
 		},
